<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.34.12-Prizren">
  <identifier>https://services-eu1.arcgis.com/ZOVTrLw470SDTARs/arcgis/rest/services/Catastro_(VP)/FeatureServer</identifier>
  <parentidentifier>1a7a595a81da4c5fa1d0e38fe0fd2a40</parentidentifier>
  <language>Galego</language>
  <type>dataset</type>
  <title>Catastro do Concello de Teo</title>
  <abstract>https://services-eu1.arcgis.com/ZOVTrLw470SDTARs/arcgis/rest/services/Catastro_(VP)/FeatureServer

Esta capa foi actualizada en xullo de 2025 e forma parte do Xeoportal do Concello de Teo descargada a partir da páxina de Catastro. Ofértase con fins informativos e orientativos, e non substitúe a documentación oficial dispoñible no Concello.

A capa foi publicada por ABTEMAS como parte da asistencia técnica desenvolvida para o Concello de Teo no marco da creación do visor web e outras ferramentas de apoio á xestión urbanística.</abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <dates/>
  <fees></fees>
  <rights>Concello de Teo</rights>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["ETRS89 / UTM zone 29N",BASEGEOGCRS["ETRS89",ENSEMBLE["European Terrestrial Reference System 1989 ensemble",MEMBER["European Terrestrial Reference Frame 1989"],MEMBER["European Terrestrial Reference Frame 1990"],MEMBER["European Terrestrial Reference Frame 1991"],MEMBER["European Terrestrial Reference Frame 1992"],MEMBER["European Terrestrial Reference Frame 1993"],MEMBER["European Terrestrial Reference Frame 1994"],MEMBER["European Terrestrial Reference Frame 1996"],MEMBER["European Terrestrial Reference Frame 1997"],MEMBER["European Terrestrial Reference Frame 2000"],MEMBER["European Terrestrial Reference Frame 2005"],MEMBER["European Terrestrial Reference Frame 2014"],MEMBER["European Terrestrial Reference Frame 2020"],ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[0.1]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4258]],CONVERSION["UTM zone 29N",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",-9,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9996,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Europe between 12°W and 6°W: Faroe Islands - offshore; Ireland - offshore; Jan Mayen - onshore and offshore; Portugal - mainland - onshore and offshore; Spain - mainland - onshore and offshore; United Kingdom - UKCS offshore."],BBOX[34.91,-12,74.13,-6]],USAGE[SCOPE["Pan-European conformal mapping at scales larger than 1:500,000."],AREA["Europe between 12°W and 6°W and approximately 34°50'N to 74°10'N."],BBOX[34.91,-12.01,74.13,-6]],ID["EPSG",25829]]</wkt>
      <proj4>+proj=utm +zone=29 +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>2102</srsid>
      <srid>25829</srid>
      <authid>EPSG:25829</authid>
      <description>ETRS89 / UTM zone 29N</description>
      <projectionacronym>utm</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial crs="EPSG:25829" minz="0" minx="179769313486231570814527423731704356798070567525844996598917476803157260780028538760589558632766878171540458953514382464234321326889464182768467546703537516986049910576551282076245490090389328944075868508455133942304583236903222948165808559332123348274797826204144723168738177180919299881250404026184124858368" maxy="-179769313486231570814527423731704356798070567525844996598917476803157260780028538760589558632766878171540458953514382464234321326889464182768467546703537516986049910576551282076245490090389328944075868508455133942304583236903222948165808559332123348274797826204144723168738177180919299881250404026184124858368" dimensions="2" miny="179769313486231570814527423731704356798070567525844996598917476803157260780028538760589558632766878171540458953514382464234321326889464182768467546703537516986049910576551282076245490090389328944075868508455133942304583236903222948165808559332123348274797826204144723168738177180919299881250404026184124858368" maxx="-179769313486231570814527423731704356798070567525844996598917476803157260780028538760589558632766878171540458953514382464234321326889464182768467546703537516986049910576551282076245490090389328944075868508455133942304583236903222948165808559332123348274797826204144723168738177180919299881250404026184124858368" maxz="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
